Peter Dome

Naoaki Takatsu

CECS 347

6 March 2018

Lab 3 Debounce

Since push buttons are a form of mechanical switches, its output bounces or oscillates many times before it can reach a stable state. Since the oscillation lasts only for a split second, we have used a timer type debounce based off the “Simpledebounce.c” file where we execute a 100ms delay each time the port F (push button) handler is called.